F-X35 SDK 1.2 (Build 0.17 Release) 03/14/2006
Contents:

1. Changes since F-X35 SDK 1.2.0.16
    FX35

    F235

    F335
    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

F135

· Temporarily masking PICL - LED_DRIVER_COMM_FAILURE (tlb reports HARDWARE_CB_DED_DRIVER_COMM_ERROR (0x4000)) since it is reported unnecessarily when the scanner is powered on before the computer. 

· Zero transport stepper to subtract out any slop in Calibration Wizard focus fixture arm. 

F235

· No changes.

F335

· No changes.

PTS

· Better handling of the case of a USB board without a personality.

PakonIma

· N/A.

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK. There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.
4. Version List
	Module
	Version

	TLX.dll
	1.2.0.17

	TLXClientDemo.exe
	1.2.0.17

	TLA.dll
	1.2.0.17

	TLB.dll
	1.2.0.17

	TLC.dll
	1.2.0.17

	PTS.exe
	1.2.0.17

	PakonIma.dll
	1.31.2.5


F-X35 SDK 1.2 (Build 0.16 Beta) 02/17/2006
Contents:

1. Changes since F-X35 SDK 1.2.0.15
    FX35

    F235

    F335
    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

F135

· Final versions of F135P firmware. No major changes just clean up and tweaks.

· Fixed TrackTest.  Track test did not always pass on a F135 Plus because we weren’t taking into account the new voltage reference on a 135 Plus (affects calibration wizard interface only).

· Zeroing lens stepper of focus fixture when changing directions so the slop in the lens arm is subtracted out (affects calibration wizard interface only).

F235

· No changes.

F335

· No changes.

PTS

· Better handling of the case of a USB board without a personality.

PakonIma

· N/A.

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK. There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.
4. Version List
	Module
	Version

	TLX.dll
	1.2.0.16

	TLXClientDemo.exe
	1.2.0.16

	TLA.dll
	1.2.0.16

	TLB.dll
	1.2.0.16

	TLC.dll
	1.2.0.16

	PTS.exe
	1.2.0.16

	PakonIma.dll
	1.31.2.5


F-X35 SDK 1.2 (Build 0.15 Beta) 02/07/2006
Contents:

1. Changes since F-X35 SDK 1.2.0.14
    FX35

    F235

    F335
    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

F135

· Changed variable names for Dmin to Tmax. No affect on function.

· Now settings motor speed every time before starting DX.

F235

· Changed variable names for Dmin to Tmax. No affect on function.

F335

· Changed variable names for Dmin to Tmax. No affect on function.

PTS

· Select first in combo box if USB board personality isn't written..

· Personality defaults to F235 FIFO when it isn't written, so make sure the model is a 235 before setting personality to FIFO.
· Change LED and Scanline from Control to UserControl..

· Decipher ErrorCode for TLX defined COM errors.

· Set LED red if there is an TLX error callback as well as a COM error.
· Implement cancel scan for four channel save.
· Set pass for minimum pixel value to 50% of max.
· Validate Ir light, but drop limit to 8000 instead of 32000 for RGB light.
· Set currently selected tab after test is completed.
PakonIma

· N/A.

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK. There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.
4. Version List
	Module
	Version

	TLX.dll
	1.2.0.15

	TLXClientDemo.exe
	1.2.0.15

	TLA.dll
	1.2.0.15

	TLB.dll
	1.2.0.15

	TLC.dll
	1.2.0.15

	PTS.exe
	1.2.0.15

	PakonIma.dll
	1.31.2.5


F-X35 SDK 1.2 (Build 0.14 Beta) 1/25/06
Contents:

1. Changes since F-X35 SDK 1.2.0.13
    FX35

    F235

    F335
    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

F135

· Handling registry for both 135 and 135 Plus motor speeds.  TLB defaults to F135 Plus, then if it sees a 135 Pic address it reverts to the 135 data in the registry.

· Now setting default ring tail buffer sizes depending on which scanner is connected.  They are 8 MB for a 135 (as they were before) and they are bumped up to 24 MB for a 135 Plus

· TLB now defaults to 135 plus high res buffer settings.  HighRes buffer was 1300 Roll/2600 total, they are now 2400 and 4800.  These settings will work for both scanners.  If resources are limited and you are running with a 135, then you may want to use regedit to change these settings back to the 135 settings.

F235

· N/A.

F335

· N/A 
PTS

· Drive Motor commands were not working on an F135.  They are now.

· Opened up motor speed tolerances for all scanners from +/- 5% to +/- 10% of nominal

· Opened up 3x10 matrix  tolerance for all scanners from +/- .15 to +/- .2  of identity(1). This is for the diagonal only.

· Added support of 135 Plus scanners such as EEPROM checking, firmware loading, motor commands, etc.

· Now showing hardware version 100 as a production version (some early runs of 135/335 were set to hw version 100).

· Fixed bug where if you tried a command that was not supported by the scanner, PTS would get in bad state then not work (always gave error even for supported commands)
· If you ran stepper test on a 135 you would get an error, which is OK, but if you then connected a 235 the stepper test would fail for that to.  You had to shutdown PTS and restart in order to do stepper test on a 235 after you do it on a 135.  Now you can go from 135 stepper test to 235 stepper test without closing and reopening PTS.

PakonIma

· N/A.

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK.

There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.
4. Version List
	Module
	Version

	TLX.dll
	1.2.0.14

	TLXClientDemo.exe
	1.2.0.14

	TLA.dll
	1.2.0.14

	TLB.dll
	1.2.0.14

	TLC.dll
	1.2.0.14

	PTS.exe
	1.2.0.14

	PakonIma.dll
	1.31.2.5


F-X35 SDK 1.2 (Build 0.13 Beta) 1/16/06
Contents:

1. Changes since F-X35 SDK 1.1.37.12
    FX35

    F235

    F335
    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

F135

· LoadImageFromBuffer source rectangle flipping is slightly optimized

· Bug 719 – EC_TimeOut at end of scan.  If low end computer is heavily loaded sometimes time out would occur while waiting for scan to complete. Changed time out from 3 to 6 seconds.

F235

· Bug 719 – EC_TimeOut at end of scan.  If low end computer is heavily loaded sometimes time out would occur while waiting for scan to complete. Changed time out from 3 to 6 seconds.

· Bug 702 - CalibrationWizard interface was not setting gain and offset on CCD so PTS light test display showed light iwthout gain applied.  Because OEMs and PSI do not use CalibrationWizard interface, this bug only affected PTS.

F335

· Bug 719 – EC_TimeOut at end of scan.  If low end computer is heavily loaded sometimes time out would occur while waiting for scan to complete. Changed time out from 3 to 6 seconds.

PTS

PakonIma

· Built with IMA June 2006 6.0 libraries.

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK.

There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.
4. Version List
	Module
	Version

	TLX.dll
	1.2.0.13

	TLXClientDemo.exe
	1.2.0.13

	TLA.dll
	1.2.0.13

	TLB.dll
	1.2.0.13

	TLC.dll
	1.2.0.13

	PTS.exe
	1.2.0.13

	PakonIma.dll
	1.31.2.5


F-X35 SDK 1.1 (Build 36.12 Release) 12/15/05

Contents:

1. Changes since F-X35 SDK 1.1.36.11
    FX35

    F235

    F335
    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35


Bug 709 - Reference Manual states ColorPortraitMode is not implemented

Bug 711 - Installer was installing CrystalReports merge modules that aren't used

F135

F235


Bug 707 - F235 Col Neg Scan shows artifacts in green/blue channels

F335


Bug 712 - TLC hardware callback not translated to TLX hardware callbacks
PTS 


Bug 710 - DX Alignment test failed with error WaitForLampTemperatureStable

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK.

There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.
BUG 702 – PTS Light test displays light without the gain applied
BUG 704 - Redistributable installer does not upgrade 1.0 redistributable

4. Version List
	Module
	Version

	TLX.dll
	1.1.36.12

	TLXClientDemo.exe
	1.1.36.12

	TLA.dll
	1.1.36.12

	TLB.dll
	1.1.36.12

	TLC.dll
	1.1.36.12

	PTS.exe
	1.1.36.12

	PakonIma.dll
	1.31.1.4


F-X35 SDK 1.1 (Build 36.11 Beta) 11/21/05

Contents:

1. Changes since F-X35 SDK 1.1.36.10
    FX35

    F235

    F335

    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35


Bug 695 - TLXClientDemo does not see MFC 7.1 dll's

F135


Bug 700 - 'PutScannerInfoPreFrameUser' is not working as expected on an F135 


Bug 697 - PICM firmware upload fails

F235

F335

PTS 

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK.

There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.

4. Version List
	Module
	Version

	TLX.dll
	1.1.36.11

	TLXClientDemo.exe
	1.1.36.11

	TLA.dll
	1.1.36.11

	TLB.dll
	1.1.36.11

	TLC.dll
	1.1.36.11

	PTS.exe
	1.1.36.11

	PakonIma.dll
	1.31.1.4


F-X35 SDK 1.1 (Build 36.10 Beta) 10/26/05

Contents:

1. Changes since F-X35 SDK 1.1.35.9
    FX35

    F235

    F335

    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

F135

F235

F335

PTS – BUG 690 – Track does not work (results indicate red light even though test passed)

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK.

There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0 or 1.1.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.

4. Version List
	Module
	Version

	TLX.dll
	1.1.36.10

	TLXClientDemo.exe
	1.1.36.10

	TLA.dll
	1.1.36.10

	TLB.dll
	1.1.36.10

	TLC.dll
	1.1.36.10

	PTS.exe
	1.1.36.10

	PakonIma.dll
	1.31.1.4


F-X35 SDK 1.1 (Build 35.9 Beta) 10/26/05

Contents:

1. Changes since F-X35 SDK 1.1.33.7
    FX35

    F235

    F335

    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

· Version info for all files set the same. (i.e. 1.1.35.9)

· New PICL and PICM firmware for F135 with improved DX reading

· Adds Pakon Troubleshooter Software (PTS) for troubleshooting Pakon scanners.

F135

· BUG 688 TLB and TLC do not write Color calibration data to registry
F235

· BUG 694  TLA not sensing APS cartride in F235C
F335

· BUG 685 EC_PFS_WritePastEOF not handeled exactly right
· BUG 688 TLB and TLC do not write Color calibration data to registry
· Allowable range for LampDelayOff changed from 20 sec to 180 sec. 

· Allowable range for AmbientTempRecalSwing changed from +/-2 deg C to +/-6 deg C. (change request to help with long roll scanning)

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK.

There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.

4. Version List
	Module
	Version

	TLX.dll
	1.1.35.9

	TLXClientDemo.exe
	1.1.35.9

	TLA.dll
	1.1.35.9

	TLB.dll
	1.1.35.9

	TLC.dll
	1.1.35.9

	PakonIma.dll
	1.31.1.4


F-X35 SDK 1.0 (Build 33.7 Release) 10/10/05

Contents:

1. Changes since F-X35 SDK 1.0.1.5
    FX35

    F235

    F335

    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
FX35

· Version info for all files set the same. (i.e. 1.0.33.7)

· Color Negative and BnW image data path enhanced.  Final sRGB images or less noisy and more contrast has been added (EBP algorithm).  Affects color path for all scanner types.  This only affects SDK users that are saving with the SAV_UseColorSceneBalance save option.

· Removed the dependancy on a resource.hm file from the TLXClientDemo project

· Added hooks for simulator version of software installation.

· Included legacy driver files so after un-installing F135 SDK, F235 SDK or F335 SDK and installing FX35 SDK, the scanner driver loads properly.

· New Lamp Board Firmware for F335 to eliminate erroneous fan slow errors logged in error log

· New APS firmware for F235C and F335C with Improved CM1 reading in presence of CM2 data 

F135
F235

F335

· Allowable range for LampDelayOff changed from 20 sec to 180 sec. 

· Allowable range for AmbientTempRecalSwing changed from +/-2 deg C to +/-6 deg C. (change request to help with long roll scanning)

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK.

There is no need to recompile the client when upgrading an existing installation of the FX35 SDK 1.0.

3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.

4. Version List
	Module
	Version

	TLX.dll
	1.0.33.7

	TLXClientDemo.exe
	1.0.33.7

	TLA.dll
	1.0.33.7

	TLB.dll
	1.0.33.7

	TLC.dll
	1.0.33.7

	PakonIma.dll
	1.31.1.4


F-X35 SDK 1.0 (Build 1.5 Release) 07/8/05

Contents:

1. Changes since F-X35 SDK 1.0.0.4
    FX35

    F235

    F335

    F135

2. Installation

3. Known Problems

4. Version List

1. Changes in this release
· RollId parameter is now fully implemented.
· If APS Film ID not read properly, Film ID gets set to -1.  Before the film ID might look OK, but it did not match the cartridge Film id.
· Added New calls to set the Film ID of an APS roll and a new call to get the CHOL for an APS roll  (F235 and F335 only).
· Made improvements to the APS scanning by improving DX reading and FAT bit reading  (F235 and F335 only).

· New DX firmware for the F235 and F335.

2. Installation:

Remove any Pakon software (other than F-X35 SDK) currently installed on the Target Machine.

Install the F-X35 SDK
Clients should either have their applicatons call InitializeScanner with FirmwareUpdate enabled or use some other means to update the firmware on the DX board of the F235 and F335.
3. Known Problems:

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.

4. Version List
	Module
	Version

	TLX.dll
	1.0.1.5

	TLXClientDemo.exe
	1.0.1.5

	TLA.dll
	1.0.32.6

	TLB.dll
	1.0.2.14

	TLC.dll
	1.0.2.13

	PakonIma.dll
	1.31.0.3


F-X35 SDK 1.0 (Build 0.4 Release) 06/13/05

Contents:

1. Changes since F-X35 SDK 1.0.0.3
    FX35

    F235

    F335

    F135

2. Installation

3. Known Problems

4. Version List

1. Changes since F-X35 SDK 1.0.0.3
F-X35 SDK 1.0.0.4 changes (since F-X35 SDK 1.0.0.3):
Version change from 1.0.0.3 to 1.0.0.4
Installer now adds all the necessary supporting DLL’s.  Only affected SDK users using SaveToDisk with file format set to jpeg or EXIF jpeg.
F-235:

Version change from 0.0.31.3 to 0.0.31.4

BUG 669 - Motor board misses some commands and TLA does not detect
F-335:  

No changes from F-X35 SDK 1.0 (Build 0.3 Beta)
F-135:
No changes from F-X35 SDK 1.0 (Build 0.3 Beta)

PakonIMA.dll:

Changed from version 1.31.0.2 to 1.31.0.3

BUG 670 – contrast adjustment was not working. Only affected SDK users using SAV_UseColorSceneBalance and doing a PutPictureInfo to change the contrast setting.
2. Installation:

Remove any Pakon software currently installed on the Target Machine.

If you have UseLampColdStart turned off in the registry, you should turn it back on.

Install the F-X35 SDK

3. Known Problems:

RollID parameter in the TLX interface is not yet implemented.  You can pass in a RollID but you will always get 1000 back.

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.

4. Version List
	Module
	Version

	TLX.dll
	1.0.0.4

	TLXClientDemo.exe
	1.0.0.4

	TLA.dll
	31RC4

	TLB.dll
	1.0.1.13

	TLC.dll
	1.0.1.11

	PakonIma.dll
	1.31.0.3


F-X35 SDK 1.0 (Build 0.3 Beta) 05/10/05

Contents:

1. Changes

    F235

    F335

    F135

2. Installation

3. Known Problems

4. Version List

1. Changes

F-X35 SDK 1.0.0.3 changes (since F-X35 SDK 1.0.0.2):
Cleaned up some construction destruction methods to prevent memory leaks that occurred during each Advise/Unadvise cycle.

Removed the SaveToSharedMemory method from the save interface.

Added some com plumbing for more complete support of .net and multithreading.
F-235 SDK 31RC3 changes (since F-235 SDK 30RC2):

Some of the options in the F-235 interface have been removed to: make implementation easier, make implementation common with the F-135 and F-335, reduce problems with different OEM implementations.

BUG 661 - Filter wheel hardware failure is not reported by TLA/PSI

CR 647 – Use digitalice library that does not activate the thread priority time critical

CR 648 - Added abiltity to apply SBA to digital input (SAV_UseColorSceneBalanceDigital)

CR 610 - The entries in the log files “PakonErrorLogMain”, “PakonErrorLogSave” and “PakonErrorLogScan” now include the serial number, firmware info to help identify which log entries are for which scanner.  The entries also now include the error number in parenthsis so you can relate the error log to the error number you see from PSI. The logs are now in the Logs subdirectory.

CR 652 - Added Base8Ratio_HR_LR to the Scan folder of the registry.  This registry entry is 8 by default which gives a 175 X 262 pixel low res image (same as 30RC2).  The other entry accepted is 4 which will give a 350 x 525 pixel low res image.

CR 650 - Implemented iLampSaverSec parameter in the Get and PutScannerInfo000 calls.  Sets lamp to standby voltage and filter wheel to blocked position after iLampSaverSec seconds of neither scanning nor calibrating.  This will extend the life of the Light bulb and the dyes in the CCD chip.

CR 651 - Eliminate ScanOptions related to cartridge scanning that did not work and caused confusion for SDKusers.

BUG 646 - A temporary buffer that is allocated when rendering a hi res image was twice as big as it needed to be (90 Mbytes instead of 45 Mbytes).

CR 656 - Add MOF data error correction before sending data to MOF edc library

CR 655 - Add MOF calibration sequence to Manufacturing Calibration procedure

If DX firmware indicates tail first after three or more head first reads are acquired, the tail first warning is ignored and not passed on to the client.

The DX firmware uses a USHORT counter which can cause some rollover issues.  This should be resolved now.Handling the error case where the DX sensor reports finding film immediately.  We will use the CCD for positioning in this case.

Added EC_PI_NO_DISK_SPACE which indicates a save to disk was not completed due to lack of free disk space.

Lamp warm-up is faster.

F-335 1.0.1.11 changes  (since F-335 SDK 1.0.0.9)

BUG 666 - Fixed a memory leak when saving images.

Default processed ringtail size changed from 16 Meg to 32 Meg.

BUG 664 - Eliminated the delay between WTP_CorrectionComplete and WTP_ScanningStarted which was occurring during the ScanPictures progress callback sequence.

BUG 663 - Enabling the LampDelayOff causes EC_LampWarmUpFailure

BUG 660 - EC_LampWarmUpFailure (error number 142) when doing corrections

BUG 653 - Calling ForceCorrections() with the CALIBRATE_Focus or CALIBRATE_FocusAdvanceFilm bits set did not turn on the lamp - now it does.

CR 652 - Added Base8Ratio_HR_LR to the Scan folder of the registry.  This registry entry is 8 by default which gives a 175 X 262 pixel low res image (same as 30RC2).  The other entry accepted is 4 which will give a 350 x 525 pixel low res image.

CR 648 - Added abiltity to apply SBA to digital input (SAV_UseColorSceneBalanceDigital)

BUG 654 - MOF reading fails if running debugger and SDK TLAClientDemo DebugU build

CR 656 - Add MOF data error correction before sending data to MOF edc library

CR 655 - Add MOF calibration sequence to Manufacturing Calibration procedure

F-135 changes (since F-135 SDK 1.0.0.13)
CR 648 - Added abiltity to apply SBA to digital input (SAV_UseColorSceneBalanceDigital)

2. Installation:

Remove any Pakon software currently installed on the Target Machine.

If you have UseLampColdStart turned off in the registry, you should turn it back on.

Install the F-x35 SDK

3. Known Problems:

RollID parameter in the TLX interface has been is not yet implemented.  You can pass in a RollID but you will always get 1000 back.

Operator/Developer must ensure that only one scanner is power on and connected to the computer at one time.

Only one instance of TLX may be running at one time.  Starting two applications that both load TLX can cause unstable/unexpected results.

4. Version List
	Module
	Version

	TLX.dll
	1.0.0.3

	TLXClientDemo.exe
	1.0.0.3

	TLA.dll
	31RC3

	TLB.dll
	1.0.1.13

	TLC.dll
	1.0.1.11

	PakonIma.dll
	1.31.0.2


