PSI-FX35 Installation CD Release Notes 

____________________________________________________________________
Installation Instructions:

1. Remove all currently installed Pakon software using the Add/Remove Programs in the control panel. You may need the original CD to succesfully remove the software.

2. Install the FX35 Redistributable Software.

a. Insert the CD

b. On the Windows task bar Click “Start” and then “Run”

c. Type “R:\fx35install\setup.exe”

d. Click OK and follow the instructions of the install wizard

3. Install the PSI FX35 software by .

a. Insert the CD

b. On the Windows task bar Click “Start” and then “Run”

c. Type “R:\setup.exe”

d. Click OK and follow the instructions of the install wizard

4. Start IQueue 

5. Setup IQueue

6. Start PSI

7. Setup PSI EasyOrder

PSI/IQueue II Version 2.4 Build 0.3
March 2006
Changes in this version:

Added F135 Plus Scan dialog

Includes FX35 1.2 which supports the F135 Plus

Fix bug in 2.3.0.9 Single Print method that would occassionaly casue an exception when printing.
PSI/IQueue II Version 2.3 Build 0.9
February 2006
Changes in this version:

every 24 hours, PSI cleans up the archive
Adds support for Picture Center Manager

Adds support for EZPrints Specialty products via DLSQueue

On a KPCD the OrderId is now contained in info.cd so a lab can look in Info.cd and associate a CD to an order.

Single Print method changed to queue two jobs at once in order to increase output of the printers.  This has not been tested thouroughly and likely has a bug.  Therefore 2.3.0.9 should not be used for printing service prints.
PSI/IQueue II Version 2.2 Build 0.5
December 2005
Changes in this version:

One PSI/IQueue software installation that works with any Pakon scanner.

Improved Image quality, especially on overs and unders.  Images should have more consistent dark point levels that are dark and bright white levels.  Less noise should be present in the final images as well.

Improved DX reading on all film types.
Improved APS Cartridge handling, including Print Aspect Ratio and frame number editing and improved MOF reading.

Improved Workflow screens in PSI easy order including skipping of screens with only one option and more informative messages on others.

Can now scroll through images in the order using the hi res data (double click an image and scroll using the previous next buttons.)
More menu options in the Picture context menu for greater flexibiltiy in EasyOrder.

Increased the number of print types from 3 to 6 and improved print quantity selection. Added print summary to products dialog.  Removed the Skip command.
Added Error logging for IQueue.

Improved printer status and printer monitoring in IQueue.

Enabled the FrameType command in the main menu.
Improved the image quality of pictures printed on Kodak 6800 printers.

Updated GoldenHawk to 4.0B.

New work flow options in IQueue including New Running Jobs Grid, Dual Printing, Group Jobs by Device, Pause Job at completion, and Promote Job.  See table below
	IQueue Running Grid Feature
	Description

	New Running Jobs Grid
	The running jobs grid now shows a list of output devices instead of output products.  A device may be paused and resumed.

	Dual Printing
	Singles, indexes may be setup to output on multiple devices for increased productivity

	Group Jobs by Device
	Jobs from the same order and that are output on the same device may be grouped by device to enhance order collation

	Pause Job at completion
	The job will automatically pause at completion allowing the operator to see the Roll ID for which the product is associated with.

	Promote Job
	Allows the operator to promote a job in the pending grid so it is next to be produced.

	More Information
	CD Jobs are now displayed as either Pakon CD or Kodak Picture CD.


CR 679 –Added new cdr to list of KPCD approved writers."SOHW-1693S")

Bug 676 - Archive dialog column heading use static strings that can't be translated 

Bug 640 - Switching between EasyOrder and classic view could leave the 


Frames per strip setting in an invalid state.  This could result in an


EC_InvalidParameter when leaving the Scan Dialog.

CR 639 - Color adjust dialog placement and sharpness adjust dialog placement should be 


 persistent 

CR 638 – Add PSI command “Setup->Color Preference”   

CR 637 - Add splice mode 

Bug 636 - Cropping does not mark an order as modified, so cropping does


     not always show up in prints.

Bug 595 – CD burner not visible from PSI or Windows Explorer when IQueue running.

Bug 582 - Too many files being imported EC 3012 should be handled better

Bug 575 - PSI doesn't recover well from an error code 


     EC_BufferDriveMegabytesRollTooSmall

Bug 573 - Open from Archive problems
· KIAS orders can now be opened via archive search
· Open button is disabled until valid search results
· Message box when search returns no results

